|  |  |
| --- | --- |
| ***Aircraft Dimensions*** | ***KR 020 TOPAZ*** |
| Construction Type | Full Vinyl-Ester Composite |
| Wing Span (m) | 10.58 |
| Length (m) | 5.95 |
| Height (m) | 2.35 |
| Verified Empty Weight (kg) | 310kg |
| MTOW (kg) | 560kg |

|  |  |
| --- | --- |
| ***Engine & Propeller Detail***  | ***KR 020 TOPAZ*** |
| Engine | Rotax 912 uls 100hp |
| Propeller | PESZKE 66inch 3-blade Composite |

|  |  |  |
| --- | --- | --- |
| ***Design Speeds*** | ***Km/h*** | ***Knots*** |
| VC | 200 | 108 |
| VNE | 240 | 130 |
| VSO  | 65 | 35 |

|  |  |  |
| --- | --- | --- |
| ***Performance Values*** | ***Metres*** | ***Feet*** |
| Climb Rate @ Sea Level | 8m/s | 1550 ft/min |
| Take-Off Distance | 70m | 230ft |
| Landing Distance | 100m | 328ft |

|  |  |
| --- | --- |
| ***Technical Specifications*** | ***KR 020 TOPAZ*** |
| Fuel Capacity | 86 Litre Wing Tanks |
| Fuel Consumption | 13 Litres/Hour |
| Economy Range (km) | 1300km Without Reserve |

|  |  |
| --- | --- |
| ***Standard Equipment Levels***  | ***KR 020 TOPAZ*** |
|  Flying Instrumentation | 79mm - ASI; ALT; VSI 57mm - Panel Mounted Compass; Slip, Flap & Trim Position Indicators, Strobe, Left/Right Position Lights.  |
| Mandatory AOA Alarm For PPL Training Required | Included |
| Engine Instrumentation | RPM; Oil Temperature; Oil Pressure; 2 x CHT; Fuel Level Gauges; Voltmeter; Hobbs. |
| Avionics | MGL V6 Transceiver With Dual PPT’s Sandia Mode S Transponder |
| Exterior Paint | White 2K (Inc. Matched Spinner)  |
| Interior Paint | Grey or Light Brown |
| Wheels & Spats | 500-5 6 Ply + Painted Wheel Spats |
| Brakes | Hydraulic Hand Lever Operated  |
| Seats (Leather Bolstered Optional)  | Standard Textile Upholstered |
| Safety Belts | Four Point (Red/Black/Blue) |
| Wing Step Option | N/A |
| Canopy Cover Option | Optional |
| Tow Bar Option | Optional |

|  |  |
| --- | --- |
| ***Costs*** | ***KR 020 Topaz*** |
| Total Euro Cost As Specified Above Assuming Six (6) ‘Ready to Fly’ Factory Tested Complete Aircraft  | 56 000 Euro(R950 972.00 @ R 16.98/1.00 Euro) |
| Insured Shipping Charges | 1 x 20ft & 1 x 40ft Container R 150 000.00 (Excluding Customs VAT & Duties) |
| Manufacturing Terms: | Seven Months From Deposit Date |
| Payment Terms: | 50% Deposit On Confirmed Order 50% Balance Payable Prior To Shipping **Customs VAT, Duties & Shipping Are Only Payable On Delivery**  |